Corvette Pinball		Software Revision Information

U6:	Version 2.1
	Checksum: EE21
	Date: January 24, 1996

Changes from revision L-2:

	Fixed Super Charger lamp.  It was not blinking when it was the
	next available speed part.

	Fixed ball save during buy-in.


U6:	Version L-2
	LA-2 Checksum: D902
	LX-2 Checksum: C602
	Date: October 4, 1994

Changes from revision L-1:

	Added a difficulty setting for relighting kickback.

	LT5 LOCK can no longer time out during REV mode.

	Enhanced logic on lower rev gate to better catch the ball.


U6:	Version L-1
	LA-1 Checksum: 4301
	LX-1 Checksum: 3001
	Date: September 12, 1994

Initial release to production.
